Water Quality Measuring Device

Documentation



EN2160 – Electronic Design Realization

Department of Electronic and Telecommunication Engineering

University of Moratuwa

Samaranayake M.A.S – 210559H

Wijethilaka U.G.P.M.B – 210724K

User Requirements

Water Quality Measuring Device can assess the quality of water based on several parameters such as pH value, temperature of the water, and turbidity. This device will be particularly useful in industrial settings where it can measure the quality of water discharged after factory usage.

Industrial wastewater often contains various contaminants that can be harmful to the environment and human health. Regular monitoring and assessment of water quality is therefore crucial. However, existing methods can be time-consuming, expensive, and may not provide real-time data.

Current solutions typically involve manual sampling and laboratory testing. While these methods can be accurate, they are not ideal for continuous monitoring or real-time data analysis. Some digital devices exist for this purpose, but they may not offer comprehensive data analysis or user-friendly interfaces. Meantime our device is unique because it not only measures multiple water quality parameters but also provides real-time data via a mobile application. Furthermore, it uses an AI model to analyze the data and determine the usability of the water, making it a smart solution for water quality monitoring.

The most affectable parameters of the water are following parameters. They are,

1. pH value – Define whether water is acidic or caustic.
2. Turbidity – How much amount of light can pass through water.
3. Temperature – Temperature of the water
4. Conductivity – Measures the ion contains in the water.

This device can continuously monitor the above parameters and it can predict the water is whether good to use or not, and the mobile app of the device can show the values of above parameters.

Following are the user requirements of the device.

* Cost effectiveness – usually to measure the water quality in a lab, it costs lot of chemicals, and these chemicals are bit expensive and cannot use continuously due to the higher cost, but this device can measure the water quality without any cost. The only cost is the amount that need to be paid when buying the device.
* Time effective – when you put this device into the water, you can measure the value of the above parameters within a small amount of time.
* User friendly -There are no hard calibrations or tests to use this device. Only need to dip the device little bit in the water until the values are taken.
* Size and durability – This device is a water proof device and the product enclosure is a plastic enclosure with a small size.
* Real time data monitoring – Values of the above parameters can be taken real time without any tests in labs.

Conceptual Designs

Conceptual Design 01

* The design of this device is like a cylinder, and the main four sensors of the device are located at the bottom of the device. Bottom of the device can be drowned in the water to get values. The device is water sealed. Device is integrated with a smart plug device.
* Smart Plug – This device turns off the water supply (water pump) if the water source is not in good position to use. The data for the device to work will be transferred through cloud base data management system.

|  |
| --- |
| Enclosure Design |
|  |

|  |
| --- |
| Functional Block Diagram |
|  |

Conceptual Design 02

* The design of this device is like a cylinder, and the main four sensors of the device are located at the bottom of the device. Bottom of the device can be drowned in the water to get values. The device is water sealed.

|  |
| --- |
| Enclosure Design |
|  |

|  |
| --- |
| Functional Block Diagram |
| A diagram of a system  Description automatically generated |

Conceptual Design 03

* The device enclosure is like a box type and the pH sensor is attached separately to the device. Other three sensors are integrated with the enclosure design. Device can be drowned in the water to measure values. Device is rechargeable and wireless charging is used.

|  |
| --- |
| Enclosure Design |
|  |
| Functional Block Diagram |
|  |

These are the three conceptual designs we have designed, and following are the evaluation of the these conceptual designs.

Evaluation of the Conceptual Designs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | Conceptual design 1 | Conceptual design 2 | Conceptual design 3 |
| Newly added features | | LED indicators to show the water quality status.  Smart switch for cutoff power supply  Mobile Application | Direct power charging  LED indicators to show the water quality status.  Mobile Application | Wireless Charging  pH Probe can be accessible separately.  Mobile Application |
| Removed features | | Wireless charging  pH Probe can be accessible separately. | Wireless charging  Smart Switch  pH Probe can be accessible separately. | Smart Switch  Direct Power Charging |
| Enclosure design criteria comparison | Functionality | 9 | 8 | 7 |
| Aesthetics | 8 | 8 | 7 |
| Heat dissipation | 6 | 6 | 6 |
| Assembly and serviceability | 8 | 8 | 9 |
| Ergonomics | 8 | 8 | 7 |
| Simplicity | 8 | 8 | 7 |
| Durability | 8 | 8 | 7 |
| Functional block design criteria comparison | Functionality | 8 | 9 | 7 |
| User experience | 9 | 8 | 8 |
| Manufacturing feasibility | 7 | 7 | 7 |
| Cost | 7 | 8 | 7 |
| Performance | 8 | 7 | 7 |
| Future proo1ng | 8 | 7 | 8 |
| Power | 8 | 8 | 8 |
| **Total** | | 110 | 108 | 102 |

Design Selection

According to above evaluation criteria first conceptual design has chosen to develop.

Features of the design

All the main four sensors of the device are integrated within the device and there are two indicators to show the usability of the water according to the values taken by the sensors.

User can observe the real time values through a mobile application and the mobile application can predict whether the water is usable or not.

Enclosure type of the device is cylindrical.

There is a smart plug device is integrated to the design and the smart plug work as the switch to the water pump. If the quality of the device is not in a good condition, then smart plug can automatically turn off the water pump.

|  |  |
| --- | --- |
| Enclosure Design | Functional Block Diagram |
|  |  |

PCB Schematic Design

Following pages contain the schematic design for the PCB.

PCB Design (Routing and component placement)

A computer chip with many different colored lines

Description automatically generated with medium confidence

Top Layer

A red and black circuit board

Description automatically generated

Bottom Layer


A computer circuit board with blue dots

Description automatically generated

3D View

|  |  |
| --- | --- |
|  |  |
|  | |

Enclosure Design



A transparent box with a black and grey object

Description automatically generated